Kokkinos C, Economou A. Tin film sensor with on-chip three-electrode configuration for voltammetric determination of trace Tl (I) in strong acidic media. TalantaTALANTA. 2014;125:215-220.