Tombras GS. 1-Bit delayed encoding improves continuously variable slope delta modulator performance. International Journal of Electronics [Internet]. 1992;73:549-554.