Tombras GS, Karybakas CA. Running average error reduces overload noise in delayed delta-modulation systems. International Journal of Electronics [Internet]. 1988;65:1105-1115.